# measure

public Unit measure(OnDeviceResultListener listener, ScanMode modes)

Run a measurement for the specified scan modes, or all supported scan modes if none are specified. If unsupported modes are selected, the measurement will fail with status code CommandStatus.ERROR_NOT_SUPPORTED. This method is asynchronous and will return immediately. Status of this operation is provided by the OnDeviceResultListener callback

#### Parameters

listener

Callback interface which provides the command status and measurements on completion

modes

Scan modes to select. If omitted, the device will measure for all supported modes