# MeasurementData

class MeasurementData

Class describing measurement data from a Nix device

## Constructors

MeasurementData
Link copied to clipboard
constructor()

## Types

Mini
Link copied to clipboard
class Mini(status: Byte, @Size(value = 3) scanData: DoubleArray) : MeasurementData.Pro, IMeasurementData

Class describing measurement data from a DeviceType.MINI device

Mini2
Link copied to clipboard
class Mini2(status: Byte, scanDataA: DoubleArray, scanDataB: DoubleArray, tRefInteger: Int, tScanInteger: Int, tCompEnabled: Boolean) : MeasurementData.QC, IMeasurementData

Class describing measurement data from a DeviceType.MINI2 device

Mini3
Link copied to clipboard
class Mini3(status: Byte, scanBytes: ByteArray, tRef: Float, tScan: Float, tCompEnabled: Boolean, tileEnabled: Boolean) : MeasurementData.Spectro2, IMeasurementData

Class describing measurement data from a DeviceType.MINI3 device

Pro
Link copied to clipboard
open class Pro(val status: Byte, @Size(value = 3) scanData: DoubleArray, val deviceType: DeviceType = DeviceType.PRO) : IMeasurementData

Class describing measurement data from a DeviceType.PRO device

Pro2
Link copied to clipboard
class Pro2(status: Byte, scanDataA: DoubleArray, scanDataB: DoubleArray, tRefInteger: Int, tScanInteger: Int, tCompEnabled: Boolean) : MeasurementData.QC, IMeasurementData

Class describing measurement data from a DeviceType.PRO2 device

QC
Link copied to clipboard
open class QC(val status: Byte, scanDataA: DoubleArray, scanDataB: DoubleArray, tRefInteger: Int, tScanInteger: Int, tCompEnabled: Boolean, tileEnabled: Boolean, val deviceType: DeviceType = DeviceType.QC) : IMeasurementData

Class describing measurement data from a DeviceType.QC device

Spectro2
Link copied to clipboard
open class Spectro2(val status: Byte, scanBytes: ByteArray, val mode: ScanMode, val tRef: Float, val tScan: Float, val tCompEnabled: Boolean, val tileEnabled: Boolean, val deviceType: DeviceType = DeviceType.SPECTRO2) : IMeasurementData

Class describing measurement data from a DeviceType.SPECTRO2 device

SpectroL
Link copied to clipboard
class SpectroL(status: Byte, scanBytes: ByteArray, mode: ScanMode, tRef: Float, tScan: Float, tCompEnabled: Boolean, tileEnabled: Boolean) : MeasurementData.Spectro2, IMeasurementData

Class describing measurement data from a DeviceType.SPECTROL device

Util
Link copied to clipboard
object Util