Show / Hide Table of Contents

# Interface IDensityData

Interface describing density data

###### Namespace: NixUniversalSDK

###### Assembly: NixUniversalSDK.dll

##### Syntax

    public interface IDensityData

### Properties

#### AutoIndex

Indicates which channel (0 - 3) in Value has the strongest response, with greyness override

##### Declaration

    int AutoIndex { get; }

##### Property Value

Type | Description
--- | ---
int |

#### Mode

Scan mode for this measurement

##### Declaration

    ScanMode Mode { get; }

##### Property Value

Type | Description
--- | ---
ScanMode |

#### Status

Density status for this value

##### Declaration

    DensityStatus Status { get; }

##### Property Value

Type | Description
--- | ---
DensityStatus |

#### StatusLabel

Density status label for this value

##### Declaration

    string StatusLabel { get; }

##### Property Value

Type | Description
--- | ---
string |

#### Value

Density values (4 channels, CMYK order)

##### Declaration

    double[] Value { get; }

##### Property Value

Type | Description
--- | ---
double[] |